Filter:

Submit Search

# Making adjustments to the design

Designing a fiber optic network using Comsof Fiber follows an almost fully automated workflow. Loading the GIS data to start from, generating additional features needed for the design, validating all input data and calculating the design based on the set rules do not require any manual intervention by the designer. For an optimal result, however, a small intervention may be required in some cases. It is possible that at an early stage adjustments are needed to the input side or that optimizations are required on the calculated design.

The Comsof Fiber Integration Module provides the flexibility to do both.