Filter:

Submit Search

## Configuring your templates

A workspace is created by duplicating a template structure. The template workspace defines Comsof Integration Module properties and calculation rules, and data file structure. You must create a separate workspace template for each Comsof Integration Module product version you use.

To set up your workspace template:

1. Create a root directory to hold your templates, for example:

>     data/comsof/workspaces/templates

1. Add a GPKG template for each Comsof Integration Module product version you wish to use, for example:

>     <templates>/22.2.3.46

> These can be copied from your Comsof Integration Module Fiber Designer products or from the templates directory of the Comsof Integration Module module.

3. Ensure that each template workspace includes the following files:

>     registry.properties

>     input.properties

> If missing, copy the files from the templates directory of the Comsof Integration Module module.

1. Create a rules directory and add the rules files you wish to use, for example:

>     <templates>/rules/hybrid.rules

>     <templates>/rules/hybrid_cabinet_area.rules