Filter:

Submit Search

## Configuring your application

Comsof Fiber functionality is accessed via the myWorld feature comsof_workspaces. This feature type must be made accessible to your application.

Go to the Features tab page of the Network Manager Telecom Configuration module page to make the layer comsof_workspace accessible to your Network Manager application.

For vizualization, you may also want to make the comsof_workspaces layer and the various comsof_in and comsof_out layers available. These layers are used to display the Comsof workspaces and their contents. Go to the Layers tab page of the Network Manager Telecom Configuration module page to configure the layers you want to have displayed in the map.