Filter:

Submit Search

# Installation

The following changes relate to installation and upgrade.

## Prerequisites

Component | Version | Comments
--- | --- | ---
IQGeo Platform | 7.2 | Mandatory
IQGeo Network Manager Telecom | 3.2 or 3.3 | Mandatory
Comsof Fiber | 24.2 | Mandatory

All components must include any released patches.

Comsof Fiber v.24.2 is required to ensure cable functionality works as expected (see Support re-use of existing cables).

## Installing the software

1. Uncompress the software download and copy the comsof folder into:

       <myWorld_install_dir>/WebApps/myworldapp/modules

2. Rebuild your JavaScript bundles:

       myw_product build applications

## Creating a new database

If you do not already have an IQGeo database, or that database does not yet have the Comsof Integration Module tables installed, you will need to:

- Install the Network Manager Telecom tables.

- Install the Comsof Integration Module tables.

- Configure your installation.

These processes are covered in detail in the Installation and Configuration Guide.

## Upgrading an existing database

If you already have a Network Manager Telecom database with Comsof Integration Module database from a previous release, you will need to:

- Upgrade your database (see Upgrading your database).

- Perhaps perform some post-upgrade configuration changes.

These processes are covered in detail in the Installation and Configuration Guide.

## Data mapping examples

- The example populate mappings include the export of conduits as existing pipes. This allows for the re-use of existing conduits.