Filter:

Submit Search

## Comsof Fiber warnings

When you design a network using the Comsof Fiber Integration Module, some operations may trigger warningsBelow is a (non-exhaustive) list of warnings you can encounter, with a link to the relevant topic in the Comsof Fiber Manual to help you understand and preferably resolve the issue.

### Nodes are not connected to the rest of the area

Precise warning:

<x> nodes are not connected to the rest of the area.
Check if all streets in the input file are connected.

Topic in manual: Unconnected Nodes

### Demand points or central office are not connected to the rest of the area

Precise warning:

<x> demand points or central office locations are not connected to the rest of the area. If you continue without making corrections to the input files these points will not be taken into account in the calculation.

Topic in manual: Unconnected Nodes

### Drop point connection exceeds cut-off distance

Precise warning:

The following Drop Points have a connection to their Distribution Point that exceeds the cut-off distance (500 m): <x>

Topic in manual: Distribution - Clustering

### Distribution point connection exceeds cut-off distance

Precise warning:

The following Distribution Points have a connection to their Feeder Point that exceeds the cut-off distance (5000 m): <x>

Topic in manual: Feeder - Clustering

### Maximum blow distance violated

Precise warning:

Maximum blow distance violated: <x>

Topic in manual: Blow Distance Violated