Filter:

Submit Search

## Configuring your templates

A workspace is created by duplicating a template structure. The template workspace defines Comsof Fiber properties and calculation rules, and data file structure. You must create a separate workspace template for each Comsof Fiber product version that you plan to use.

To set up your workspace template:

1. Create a root directory to hold your templates, for example:

>     data/comsof/workspaces/templates

1. Add a GPKG template for each Comsof Fiber product version you wish to use, for example:

>     <templates>/24.2.3.87

> These can be copied from the Comsof Fiber products you may already have or from the templates directory of the Comsof Fiber Integration Module.

3. Ensure that each template workspace includes the following files:

>     registry.properties

>     input.properties

> If missing, copy the files from the `templates` directory of the Comsof Fiber Integration Module.

1. Create a rules directory and add the rules files you wish to use, for example:

>     <templates>/rules/rules.rules

>     <templates>/rules/hybrid.rules

>     <templates>/rules/hybrid_cabinet_area.rules