Filter:

Submit Search

## Making adjustments to the design

Designing a fiber optic network using Comsof Fiber follows an almost fully automated workflow. Loading the GIS data to start from, generating additional features needed for the design, validating the input data and calculating the design based on the settings in the Rules file, all these require little or no manual intervention by the designer. Yet, to achieve the most optimal result, a number of iterations are often necessary, involving manual adjustments on specific features, on clusters or network layers.

The Comsof Fiber Integration Module provides the flexibility to do carry out optimisations at an early stage in the design process to fine-tune input data or at the later stages to optimize the calculated design.

See the topics below for more information.

Topics in this section include: