Filter:

Submit Search

# Connectivity Engine Implementation

## Components

The Connectivity Engine actually comprises two components.

First, it provides the engine itself, which carries out the connectivity adjustments ("transformations") on the design as specified in the configuration settings. The way it has been implemented also provides a framework for the IQGeo Delivery staff to easily extend its functionality with customizations.

Next, there is a dedicated setting in the Advanced Settings of the Network Manager Telecom Configuration module that allows configuring different transformer settings in a uniform and structured way using JSON:

    comsof.connectivity_engine_config.<custom>

The extension <custom> can be replaced with a string of your choice, which makes it possible to have multiple settings with different configurations. Comsof Fiber Integration Module comes with a .default setting that can serve as an example or as the starting point for the configuration of customer-specific settings.

## Connectivity aspects supported by standard implementation

The standard implementation of the Connectivity Engine is capable of handling the following connectivity aspects:

- creation of patch panels in specific structures

- connectivity for existing straight-through fiber connections

- connectivity of fibers on Multi-port Terminals

- processing of reserved and unused fibers