Filter:

Submit Search

## Comsof Fiber errors

When you design a network using the Comsof Fiber Integration Module, some operations may trigger warningsBelow is a (non-exhaustive) list of warnings you can encounter, with a link to the relevant topic in the Comsof Fiber Manual to help you understand and preferably resolve the issue.

### No path found for customer node

Precise warning:

No path found for customer node <x>

This error message typically occurs while pre-processing the workspace, specifically when generating drop trenches. It indicates that there is no trench present near the node (the demand point) to which a drop trench can be laid. So to resolve this issue, a trench is needed near the node. Since trenches are typically generated from street center lines, it is important that the corresponding street center line is present in the Network Manager Telecom database and has been loaded into the workspace during populating.