Filter:

Submit Search

# Configuring the input.properties settings

When loading, editing and/or calculating input data for the workspace, Comsof Fiber functions are used. Each of these functions uses a set of parameters and settings that help determine what the outcome will look like. These parameters, which are stored in the input.properties file, are assigned default values, but can be modified to produce a different result.

For additional information on the input.properties parameters and settings, refer to the topic Input.properties File in the Comsof Fiber Manual. For detailed information on the settings of a specific function, read the relevant topic in the Comsof Fiber Manual.

To view/edit settings in the input.properties to be used on a workspace:

1. Select the workspace and make sure it has been initialized.

   1. On the map, select the parent design odf the workspace by clicking on it.

      The design turns red and the Details tab displays its name, the additional attributes and the toolbar with features to manage the design.

   2. Open the design by clicking the on the toolbar.

      The information on the design is opened in the Details tab.

   3. In the Workspaces section, click the name of the workspace you want to edit.

      The Details pane displays the information related to the workspace.

   4. Open the workspace.

      The Workspace dialog opens presenting the different operations you can have executed.

   5. Click Run to execute the operation.

      When the operation has completed, the View input.properties button becomes accessible in the Details pane.

2. Click View input.properties.

   The View / Edit input.properties dialog opens in read-only mode.

3. Click the Edit button if you want to make changes or add (a) setting(s).

4. Make the necessary changes to the file.

5. Save your changes.

6. Close the dialog.

You can now carry out the rest of the operations in the Workspace dialog with the adjusted input.properties parameters.