Filter:

Submit Search

# 2: Upgrading

# Upgrading

## Upgrading your database

Ensure IQGeo Platform has been upgraded to 7.2 and Network Manager Telecom Core has been upgraded to 3.2.

To upgrade from the previous release of Network Manager Telecom Comsof Integration Module:

Apply the Comsof upgrade:

myw_db <db_name> upgrade comsof 723215

## Post upgrade actions

After upgrading your database, for any custom Comsof populate or import mappings you should use the Settings configuration page to edit:

- Any custom Comsof populate mappings to include IN_AerialDropConnections feature_types, mapped to a src_feature_type of oh_drop route.

- Any custom Comsof import mappings to include a oh_drop_routes feature type with a filter of 'AERIALDROP' and a oh_route feature type with a filter of 'AERIAL' only, both mapped to a src_feature_type of OUT_UsedSegments.

- Additional import mappings can be configured, depending on how you would like existing cables to be mapped (the default is fiber_cable).